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COSHH ASSESSMENT
Clarke Motor Oil SAE 10W/30
	DOCUMENT INFORMATION

	Document Reference
	COSHH_25

	Issue Number
	2

	Issue Date
	25 September 2026

	Next Review
	1 June 2027

	Assessor
	Sean Ashton (Onyx Operations)

	Approved By
	Aaron Mason, Director


	Key references
▸  Clarke-API-SF-10W-30-Motor-Oil-3050845.pdf — Manufacturer Safety Data Sheet
▸  Clarke-API-SF-10W-30-Motor-Oil-3050845.pdf — Manufacturer Safety Data Sheet
▸  Clarke International sheet for API SF 10W-30 Motor Oil, article 3050845, version 4 of 11/10/2024, filed 27/09/2026. It records the product as not classified, against H315 and H411 printed on Clarke's own label for the same article. The classification in this assessment is taken from the label.
▸  Van Packs portal — COSHH section — synchronised copy carried by every operative



1. Product Identification
	Product name
	Clarke Motor Oil SAE 10W/30, API SF, 1 litre — article 3050845

	Part number
	3050845

	Supplier
	Clarke International, Hemnall Street, Epping, Essex CM16 4LG

	Pack
	1 litre

	Specification
	API SF. For 4-stroke petrol engines — pressure washers, generators, mowers and yard plant

	Active ingredients / CAS
	Severely hydrotreated / solvent-refined mineral base oil plus proprietary performance additives CAS: 64742-54-7 / 64742-65-0 (typical base stocks)

	Physical form
	Liquid

	Appearance / odour
	Amber viscous oil, characteristic mild odour

	Use
	Engine oil top-up and oil changes on the AMWS fleet and yard plant

	Location
	Jason May's COSHH cabinet, AMWS yard


2. Hazard Classification
	Overall classification: Classified under GB CLP. Skin Irrit. 2 and Aquatic Chronic 2 per the container label. Used engine oil is more hazardous still — it accumulates polycyclic aromatic hydrocarbons and is treated as a skin carcinogen, so every drain-down is the hazardous operation even though the classification below is for the fresh product.
Signal word: Warning
Hazard statements (H-codes)
H315  Causes skin irritation.
H411  Toxic to aquatic life with long lasting effects.
Precautionary statements (P-codes)
P264  Wash hands thoroughly after handling.
P273  Avoid release to the environment.
P280  Wear protective gloves and eye protection.
P302+P352  IF ON SKIN: wash with plenty of water.
P332+P313  If skin irritation occurs: get medical advice.
P362  Take off contaminated clothing and wash it before reuse.
P391  Collect spillage.
P501  Dispose of contents and container to an authorised waste-oil contractor.
GHS pictograms
•  Harmful
•  Dangerous for environment


3. Persons at Risk
4. Routes of Exposure
•  Inhalation: Negligible at ambient temperature. Oil mist only where sprayed or hot
•  Skin contact: The main route. Repeated or prolonged contact causes dermatitis. Used oil is a skin carcinogen — treat every drain-down as the hazardous operation
•  Eye contact: Transient irritation on splash
•  Ingestion: Unlikely in normal use
5. Workplace Exposure Limits
	Substance
	8-hr TWA
	15-min STEL

	Oil mist, mineral
	5 mg/m³
	10 mg/m³


6. Frequency and Duration of Exposure
COSHH Regulation 6(2) requires the assessment to consider the amount, the level and the duration of exposure.
	Amount used
	Times per day
	Duration per use

	Medium — litres
	1–5 times per day
	6–30 minutes


7. Control Measures — Hierarchy of Controls
Elimination / substitution
- Not practicable — the oil grade is specified by the engine manufacturer
Engineering controls
•  Drain pan and funnel for every oil change
•  Bunded storage in the COSHH cabinet
•  Spill kit within reach of the working position
Administrative controls
•  No hand-washing in oil or solvent — soap and water only
•  Skin checks form part of the health-surveillance conversation under SOP 8.7
•  Used oil never decanted into unmarked containers
Personal Protective Equipment (PPE)
8. Storage
	Temperature
	Ambient

	Location
	Yard COSHH cabinet, bunded

	Avoid
	Strong oxidisers; contact with food and drink

	Container
	Original container, closed, clearly labelled


9. Emergency Procedures
First aid
	Route
	Action

	Eyes
	Rinse with clean water for several minutes, eyelids held open. Get medical advice if irritation persists.

	Skin
	Wash with soap and water. Do not use solvent or abrasive hand cleaner. Remove contaminated clothing and wash it before reuse. The product is a skin irritant — get medical advice if irritation continues after washing.

	Inhalation
	Not applicable in normal use. Move to fresh air if mist has been generated.

	Ingestion
	Rinse mouth. Do not induce vomiting. Seek medical advice.


Spillage
Absorb with proprietary oil absorbent or sand. Protect the nearest drain first. The product is H411 — toxic to aquatic life with long lasting effects, so any release reaching the yard gully, a drain or a watercourse is a reportable environmental incident: report on FORM_ENV_01 and notify the Environment Agency incident hotline 0800 80 70 60. Dispose of the absorbent as hazardous waste. See SOP 9.3.
Fire
Combustible when heated. Foam, dry powder or CO₂. Do not use a water jet.
Emergency contacts
•  Emergency services: 999
•  NHS non-emergency: 111
•  AMWS supervisor: Jason May
•  HSQE support: Sean Ashton (Onyx Operations)
•  Environment Agency incident hotline: 0800 80 70 60 — if product reaches a drain, ditch or watercourse
10. Waste Disposal
Fresh oil: EWC 13 02 05*. Used oil: hazardous waste, EWC 13 02 05\* — authorised waste-oil contractor only, with a consignment note retained.
11. Risk Rating
Risk = Severity × Likelihood (S × L = R). See POL_HSQE_21 Risk Assessment policy for the full scoring matrix.
	Before controls  —  Moderate
	With controls  —  Low (residual)


12. Training Requirements
•  Safe handling and decanting
•  Dermatitis awareness and skin checks
•  Spill response — SOP 9.3
•  Used-oil handling and the carcinogen risk
13. Monitoring & Review
•  Weekly COSHH cabinet inspection by the Site Supervisor
•  Annual COSHH review, or sooner on change of product, supplier or task
•  Review immediately if the SDS obtained differs from the label classification recorded above
14. References
•  POL_HSQE_08 — COSHH Policy
•  POL_HSQE_19 — Personal Protective Equipment (PPE) Policy
•  SOP 8.5 — Hazardous Substances (COSHH)
•  SOP 8.7 — Health Surveillance
•  APP_09 — COSHH Assessments Log
•  HSE COSHH Regulations 2002 (SI 2002/2677, as amended)
•  HSE EH40/2005 Workplace Exposure Limits
•  CLP Regulation (EC) No 1272/2008 (as retained in UK law)
This assessment must be reviewed annually or sooner if circumstances change. For the full management-system context (SOPs, Appendices, policies) see the AMWS IMS portal.
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