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COSHH ASSESSMENT
Grundo-Oil (pneumatic mole / hammer lubricant)
	DOCUMENT INFORMATION

	Document Reference
	COSHH_26

	Issue Number
	1

	Issue Date
	8 September 2026

	Next Review
	1 June 2027

	Assessor
	Sean Ashton (Onyx Operations)

	Approved By
	Aaron Mason, Director


	Key references
▸  GRUNDO-OIL-TT-Technologies-206115-USA-version.pdf — Manufacturer Safety Data Sheet
▸  TT Technologies sheet for GRUNDO-OIL, material 206115, version 2-0/USA of 22/04/2015, filed 27/09/2026. The manufacturer's own sheet, agreeing with the container label on the polyethylene glycol base and on the product being not classified. The EU sheet against GRU2002311 and GRU2002317 has been requested from TRACTO-TECHNIK for 31/10/2026.
▸  Van Packs portal — COSHH section — synchronised copy carried by every operative



1. Product Identification
	Product name
	TRACTO GRUNDO-OIL — lubricant for GRUNDOMAT and GRUNDORAM, part GRU2002311 (5 l) / GRU2002317 (25 l)

	Supplier
	TRACTO-TECHNIK GmbH & Co. KG, Paul-Schmidt-Strasse 2, 57368 Lennestadt, Germany

	Active ingredients / CAS
	Polyethylene glycol, with less than 5% anionic surfactant. Water-soluble. Read from the container label photographed 24/09/2026. The manufacturer’s own safety data sheet gives the same base, polyethylene glycol of mean molecular weight 200 to 600

	Physical form
	Liquid

	Appearance / odour
	Light amber oil, mild hydrocarbon odour

	Use
	In-line lubrication of GRUNDOMAT / GRUNDORAM pneumatic soil-displacement hammers used on moling and thrust-boring work

	Location
	Jason May's COSHH cabinet, AMWS yard


2. Hazard Classification
	Overall classification: To be confirmed from the SDS. Pneumatic tool oils of this type are typically either unclassified or classified for aspiration toxicity depending on viscosity.
Signal word: None required — the manufacturer classifies the product as not a hazardous substance or mixture, and the container label carries no signal word and no pictogram
Hazard statements (H-codes)
—  Not classified as hazardous in the supplied form
Precautionary statements (P-codes)
P262  Do not get in eyes, on skin or on clothing.
P280  Wear protective gloves and eye protection.
P273  Avoid release to the environment.
P501  Dispose to an authorised waste-oil contractor.


3. Persons at Risk
4. Routes of Exposure
•  Inhalation: The significant route for this product. Pneumatic tools exhaust an oil mist at the tool and at the airline connections
•  Skin contact: Repeated contact causes dermatitis
•  Eye contact: Mist and pressurised release can carry oil to the eyes
•  Ingestion: Unlikely
5. Workplace Exposure Limits
	Substance
	8-hr TWA
	15-min STEL

	Oil mist, mineral
	5 mg/m³
	10 mg/m³


6. Frequency and Duration of Exposure
COSHH Regulation 6(2) requires the assessment to consider the amount, the level and the duration of exposure.
	Amount used
	Times per day
	Duration per use

	Small — millilitres per fill
	1–5 times per day
	1–5 minutes to charge the lubricator; exposure continues while the tool runs


7. Control Measures — Hierarchy of Controls
Elimination / substitution
- Not practicable — lubrication is required for tool life and safe operation
Engineering controls
•  In-line lubricator charged rather than oil poured into the air inlet
•  Work outdoors or in open excavation — the normal working environment disperses mist
•  Airline connections checked for leaks before the shift
Administrative controls
•  Do not stand in the tool exhaust stream
•  Charge the lubricator with the airline isolated and depressurised
•  Hand-arm vibration exposure is controlled separately under SOP 8.10
Personal Protective Equipment (PPE)
8. Storage
	Temperature
	Ambient

	Location
	Yard COSHH cabinet, bunded

	Avoid
	Strong oxidisers; contamination with grit

	Container
	Original container, closed


9. Emergency Procedures
First aid
	Route
	Action

	Eyes
	Rinse with water for several minutes. Seek medical advice if a pressurised jet has contacted the eye.

	Skin
	Wash with soap and water.

	Inhalation
	Move to fresh air. Seek medical advice if breathing is uncomfortable.

	Ingestion
	Rinse mouth. Do not induce vomiting. Seek medical advice.


Spillage
Absorb with oil absorbent. Protect the excavation and the nearest drain. Dispose as hazardous waste.
Fire
Combustible when heated. Foam, dry powder or CO₂.
Emergency contacts
•  Emergency services: 999
•  NHS non-emergency: 111
•  AMWS supervisor: Jason May
•  HSQE support: Sean Ashton (Onyx Operations)
10. Waste Disposal
Hazardous waste, EWC 13 02 05*. Authorised waste-oil contractor with a consignment note.
11. Risk Rating
Risk = Severity × Likelihood (S × L = R). See POL_HSQE_21 Risk Assessment policy for the full scoring matrix.
	Before controls  —  Moderate
	With controls  —  Low (residual)


12. Training Requirements
•  Pneumatic tool lubrication procedure
•  Airline safety — isolate and depressurise before disconnecting
•  Oil mist and dermatitis awareness
•  HAVS awareness — SOP 8.10
13. Monitoring & Review
•  Weekly COSHH cabinet inspection by the Site Supervisor
•  Annual COSHH review, or sooner on change of product, supplier or task
•  Review immediately if the SDS obtained differs from the profile assumed above
14. References
•  POL_HSQE_08 — COSHH Policy
•  POL_HSQE_19 — Personal Protective Equipment (PPE) Policy
•  SOP 8.5 — Hazardous Substances (COSHH)
•  SOP 8.7 — Health Surveillance
•  APP_09 — COSHH Assessments Log
•  HSE COSHH Regulations 2002 (SI 2002/2677, as amended)
•  HSE EH40/2005 Workplace Exposure Limits
•  CLP Regulation (EC) No 1272/2008 (as retained in UK law)
This assessment must be reviewed annually or sooner if circumstances change. For the full management-system context (SOPs, Appendices, policies) see the AMWS IMS portal.
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