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COSHH ASSESSMENT
Silicone Lubricant — General Purpose (aerosol)
	DOCUMENT INFORMATION

	Document Reference
	COSHH_29

	Issue Number
	1

	Issue Date
	25 September 2026

	Next Review
	1 June 2027

	Assessor
	Sean Ashton (Onyx Operations)

	Approved By
	Aaron Mason, Director


	Key references
▸  3975823.pdf — Manufacturer Safety Data Sheet
▸  Reached through a distributor copy because the CRC document server would not open. Records Danger, H222, H229, H315, H336, H411, matching the container label read on 24/09/2026. Not held locally — save a copy to docs/coshh/sds/. Owner: Leanne Mason, target 31/10/2026.
▸  Van Packs portal — COSHH section — synchronised copy carried by every operative



1. Product Identification
	Product name
	Ambersil Silicone Lubricant — General Purpose (aerosol), 500 ml

	Supplier
	CRC Industries UK (Ambersil). WRAS Approved Product Licence No. 1811507

	Active ingredients / CAS
	Polydimethylsiloxane in a hydrocarbon solvent carrier with liquefied petroleum gas propellant. The container label states: hydrocarbons, C7, n-alkanes, isoalkanes, cyclics CAS: 63148-62-9 (PDMS), 68476-86-8 (LPG propellant)

	Physical form
	Aerosol

	Appearance / odour
	Clear liquid spray, faint solvent odour

	Use
	General-purpose lubrication and release — hinges, seals, cable, sliding mechanisms, valve spindles

	Location
	Jason May's COSHH cabinet, AMWS yard


2. Hazard Classification
	Overall classification: Aerosol 1, with skin irritation, narcotic effects and chronic aquatic toxicity. Read from the container label photographed 24/09/2026. The supplier sheet records the same classification. The hazard is the hydrocarbon carrier and the propellant rather than the silicone itself.
Signal word: Danger
Hazard statements (H-codes)
H222  Extremely flammable aerosol.
H229  Pressurised container: may burst if heated.
H315  Causes skin irritation.
H336  May cause drowsiness or dizziness.
H411  Toxic to aquatic life with long lasting effects.
Precautionary statements (P-codes)
P210  Keep away from heat, sparks, open flames and hot surfaces. No smoking.
P211  Do not spray on an open flame or other ignition source.
P251  Do not pierce or burn, even after use.
P261  Avoid breathing spray.
P271  Use only outdoors or in a well-ventilated area.
P273  Avoid release to the environment.
P280  Wear protective gloves.
P302+P352  IF ON SKIN: wash with plenty of water.
P332+P313  If skin irritation occurs: get medical advice.
P391  Collect spillage.
P410+P412  Protect from sunlight. Do not expose to temperatures exceeding 50 °C.
P501  Dispose of contents and container to an authorised waste contractor.
GHS pictograms
•  Flammable
•  Harmful
•  Dangerous for environment


3. Persons at Risk
4. Routes of Exposure
•  Inhalation: The main route. Spray mist and solvent vapour, particularly in a chamber or van
•  Skin contact: Mild defatting on repeated contact
•  Eye contact: Irritation from direct spray
•  Ingestion: Not a realistic route from an aerosol
5. Workplace Exposure Limits
	Substance
	8-hr TWA
	15-min STEL

	Hydrocarbon solvent carrier
	Product-specific — confirm from the SDS
	Product-specific

	LPG propellant
	1000 ppm
	1250 ppm


6. Frequency and Duration of Exposure
COSHH Regulation 6(2) requires the assessment to consider the amount, the level and the duration of exposure.
	Amount used
	Times per day
	Duration per use

	Small — millilitres
	1–5 times per day
	1–5 minutes


7. Control Measures — Hierarchy of Controls
Elimination / substitution
- Use a brush-applied or wipe-on lubricant where the application allows — it removes the aerosol and the propellant entirely
Engineering controls
•  Use outdoors or in the open yard
•  Not to be used in a chamber, manhole or any confined space — the propellant is heavier than air and displaces it. See SOP 8.12
Administrative controls
•  Kept in the COSHH cabinet, away from heat
•  Never stored in a vehicle in warm weather — the container can burst above 50 °C
•  No hot work in the vicinity while spraying
•  Cans not pierced or crushed, even when empty
Personal Protective Equipment (PPE)
8. Storage
	Temperature
	Below 50 °C — do not leave in a van in summer

	Location
	Yard COSHH cabinet, away from ignition sources

	Avoid
	Heat, direct sunlight, sparks, open flame

	Container
	Original pressurised container


9. Emergency Procedures
First aid
	Route
	Action

	Eyes
	Rinse cautiously with water for several minutes. Remove contact lenses if present.

	Skin
	Wash with soap and water.

	Inhalation
	Move to fresh air and keep at rest. Seek medical advice if drowsiness or dizziness persists.

	Ingestion
	Not a realistic route. Rinse mouth if contact occurs.


Spillage
Ventilate. Eliminate ignition sources. Absorb any liquid with inert absorbent. Dispose as hazardous waste.
Fire
Extremely flammable aerosol. Do not spray towards an ignition source. Containers may burst if heated — cool with water spray from a protected position.
Emergency contacts
•  Emergency services: 999
•  NHS non-emergency: 111
•  AMWS supervisor: Jason May
•  HSQE support: Sean Ashton (Onyx Operations)
10. Waste Disposal
Hazardous waste — pressurised container, EWC 16 05 04*. Authorised contractor. Do not put in general waste, even when empty.
11. Risk Rating
Risk = Severity × Likelihood (S × L = R). See POL_HSQE_21 Risk Assessment policy for the full scoring matrix.
	Before controls  —  Moderate
	With controls  —  Low (residual)


12. Training Requirements
•  Aerosol safety and the confined-space prohibition
•  Storage temperature — the van issue
•  Waste route for pressurised containers
13. Monitoring & Review
•  Weekly COSHH cabinet inspection by the Site Supervisor
•  Annual COSHH review, or sooner on change of product, supplier or task
•  Review immediately if the SDS obtained differs from the profile assumed above
14. References
•  POL_HSQE_08 — COSHH Policy
•  POL_HSQE_19 — Personal Protective Equipment (PPE) Policy
•  SOP 8.5 — Hazardous Substances (COSHH)
•  SOP 8.7 — Health Surveillance
•  APP_09 — COSHH Assessments Log
•  HSE COSHH Regulations 2002 (SI 2002/2677, as amended)
•  HSE EH40/2005 Workplace Exposure Limits
•  CLP Regulation (EC) No 1272/2008 (as retained in UK law)
This assessment must be reviewed annually or sooner if circumstances change. For the full management-system context (SOPs, Appendices, policies) see the AMWS IMS portal.

COSHH_29 — Silicone Lubricant — General Purpose (aerosol) · Issue 1 · 25 September 2026	Page  of 
d2b6b118bf66158c8730411d5e7b60704c4e0338.jpg
Water
A Services
;| Ltd




