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COSHH ASSESSMENT
EVO TOOL Temporary Linemarking Paint — Blue
	DOCUMENT INFORMATION

	Document Reference
	COSHH_32

	Issue Number
	1

	Issue Date
	5 October 2026

	Next Review
	1 June 2027

	Assessor
	Sean Ashton (Onyx Operations)

	Approved By
	Aaron Mason, Director


	Key references
▸  No safety data sheet is held for this colour. The EVO TOOL sheet covering the range has been requested from CID Group (Site Supplies & Janitorial) — owner Sean Ashton, target 31/10/2026.
▸  Van Packs portal — COSHH section — synchronised copy carried by every operative



1. Product Identification
	Product name
	EVO TOOL Temporary Linemarking Paint — Blue

	Supplier
	CID Group — Site Supplies & Janitorial (EVO TOOL)

	Product code
	LM00110

	Active ingredients / CAS
	Acrylic resin, pigments and fast-drying solvents in an aerosol propellant. Free from propane, butane, lead and cadmium (manufacturer's specification sheet). CAS: mixture — see safety data sheet

	Physical form
	Aerosol, 750 ml can (pack of 12)

	Appearance / odour
	Blue spray

	Use
	Temporary blue line-marking for site demarcation and services


2. Hazard Classification
	Overall classification: Flammable Aerosol Cat 1, Aspiration Hazard Cat 1, Skin Irritation Cat 2, Eye Irritation Cat 2, STOT SE 3 (narcotic effects), Aquatic Chronic Cat 2
Signal word: Danger
The EVO TOOL range shares one formulation across its colours, so the same classification is applied to every colour AMWS holds. It is set at the most protective of the classifications previously recorded for these products, pending the manufacturer's sheet from CID Group.
Hazard statements (H-codes)
H222  Extremely flammable aerosol.
H229  Pressurised container: may burst if heated.
H304  May be fatal if swallowed and enters airways.
H315  Causes skin irritation.
H319  Causes serious eye irritation.
H336  May cause drowsiness or dizziness.
H411  Toxic to aquatic life with long lasting effects.
Precautionary statements (P-codes)
P210  Keep away from heat, hot surfaces, sparks, open flames and other ignition sources. No smoking.
P211  Do not spray on an open flame or other ignition source.
P251  Do not pierce or burn, even after use.
P261  Avoid breathing dust/fume/gas/mist/vapours/spray.
P280  Wear protective gloves/protective clothing/eye protection/face protection.
P410+412  Protect from sunlight. Do not expose to temperatures exceeding 50 °C.
P501  Dispose of contents/container to an authorised waste contractor in accordance with local regulations.
GHS pictograms
•  Flammable
•  Harmful
•  Human Health
•  Dangerous for environment


3. Persons at Risk
•  Line-marking operatives
•  Site personnel
4. Routes of Exposure
•  Inhalation: Vapour/mist — may cause dizziness
•  Skin contact: Irritation on prolonged contact
•  Eye contact: Irritation
•  Ingestion: Aspiration hazard
5. Workplace Exposure Limits
No UK Workplace Exposure Limits (HSE EH40/2005) assigned to this product or its constituents.
6. Frequency and Duration of Exposure
COSHH Regulation 6(2) requires the assessment to consider the amount, the level and the duration of exposure.
	Amount used
	Times per day
	Duration per use

	Small — millilitres
	1–5
	6–30 minutes


7. Control Measures — Hierarchy of Controls
Elimination / substitution
Evaluated where practicable — see Section 12.
Engineering controls
•  Use in open air wherever possible
Administrative controls
•  No smoking or hot work nearby
Personal Protective Equipment (PPE)
•  Nitrile gloves
•  Safety glasses
8. Storage
	Temperature
	Below 50 °C

	Location
	Cool ventilated store

	Avoid
	Heat, sparks, direct sunlight

	Container
	Original aerosol can


9. Emergency Procedures
First aid
	Route
	Action

	Eyes
	Rinse with water for 15 minutes. Seek medical advice.

	Skin
	Wash with soap and water.

	Inhalation
	Move to fresh air.

	Ingestion
	Do not induce vomiting. Seek immediate medical attention.


Spillage
Eliminate ignition sources. Absorb with inert material. Dispose as hazardous waste.
Fire
Flammable aerosol. Use foam, CO₂ or dry powder.
Emergency contacts
•  Emergency services: 999
•  NHS non-emergency: 111
•  AMWS supervisor: Jason May
•  HSQE support: Sean Ashton (Onyx Operations)
10. Waste Disposal
Empty aerosols are hazardous (EWC 16 05 04*).
11. Risk Rating
Risk = Severity × Likelihood (S × L = R). See POL_HSQE_21 Risk Assessment policy for the full scoring matrix.
	Before controls  —  Moderate
	With controls  —  Low (residual)


12. Training Requirements
•  Aerosol handling
13. Monitoring & Review
•  Weekly van-pack inspection
•  Annual COSHH review
14. References
•  POL_HSQE_08 — COSHH Policy
•  POL_HSQE_19 — Personal Protective Equipment (PPE) Policy
•  SOP 8.5 — Hazardous Substances (COSHH)
•  APP_09 — COSHH Assessments Log
•  HSE COSHH Regulations 2002 (SI 2002/2677, as amended)
•  HSE EH40/2005 Workplace Exposure Limits
•  CLP Regulation (EC) No 1272/2008 (as retained in UK law)
This assessment must be reviewed annually or sooner if circumstances change. For the full management-system context (SOPs, Appendices, policies) see the AMWS IMS portal.
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